ONVIFTM

Profile S Specification

Version 1.0 Rev1

November 2015

DRAFT

©2008-2015 by ONVIF: Open Network Video Interface Forum. All rights reserved.

Recipients of this document may copy, distribute, publish, or display this document so long as this copyright notice, license and disclaimer are retained with all copies of the document. No license is granted to modify this document.

THIS DOCUMENT IS PROVIDED "AS IS," AND THE CORPORATION AND ITS MEMBERS AND THEIR AFFILIATES, MAKE NO REPRESENTATIONS OR WARRANTIES, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO, WARRANTIES OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE, NON-INFRINGEMENT, OR TITLE; THAT THE CONTENTS OF THIS DOCUMENT ARE SUITABLE FOR ANY PURPOSE; OR THAT THE IMPLEMENTATION OF SUCH CONTENTS WILL NOT INFRINGE ANY PATENTS, COPYRIGHTS, TRADEMARKS OR OTHER RIGHTS.

IN NO EVENT WILL THE CORPORATION OR ITS MEMBERS OR THEIR AFFILIATES BE LIABLE FOR ANY DIRECT, INDIRECT, SPECIAL, INCIDENTAL, PUNITIVE OR CONSEQUENTIAL DAMAGES, ARISING OUT OF OR RELATING TO ANY USE OR DISTRIBUTION OF THIS DOCUMENT, WHETHER OR NOT (1) THE CORPORATION, MEMBERS OR THEIR AFFILIATES HAVE BEEN ADVISED OF THE POSSIBILITY OF SUCH DAMAGES, OR (2) SUCH DAMAGES WERE REASONABLY FORESEEABLE, AND ARISING OUT OF OR RELATING TO ANY USE OR DISTRIBUTION OF THIS DOCUMENT. THE FOREGOING DISCLAIMER AND LIMITATION ON LIABILITY DO NOT APPLY TO, INVALIDATE, OR LIMIT REPRESENTATIONS AND WARRANTIES MADE BY THE MEMBERS AND THEIR RESPECTIVE AFFILIATES TO THE CORPORATION AND OTHER MEMBERS IN CERTAIN WRITTEN POLICIES OF THE CORPORATION.

Revision history

|  |  |  |
| --- | --- | --- |
| **Vers.** | **Date** | **Description** |
| 1.0 | Dec, 2011 | First release version 1.0 |
| 1.0 Rev1 | Nov, 2015 | Clarifications following ONVIF Client Test Specification introduction.  Clarification reflecting the Device Test Specifications: Availablity of at least one ready-to-use Media Profile for Video Streaming (7.8.1). Updated document style based on recent ONVIF templates.   * Mandatory and Conditional Features have been separated in their own sections. * Requirement Tables split between Device and Client requirements. * Features have been re-ordered into a more intuitive order. |
|  |  |  |

Table of Contents

[1 Scope 5](#_Toc435301742)

[2 Normative references 5](#_Toc435301743)

[2.1 Normative References 5](#_Toc435301744)

[3 Terms and Definitions 5](#_Toc435301745)

[3.1 Definitions 5](#_Toc435301746)

[4 Technical Specification Version Requirement 5](#_Toc435301747)

[5 Requirement Levels 6](#_Toc435301748)

[6 Overview 7](#_Toc435301749)

[7 Profile Mandatory Features (normative) 8](#_Toc435301750)

[7.1 User Authentication 8](#_Toc435301751)

[7.2 Capabilities 9](#_Toc435301752)

[7.3 Discovery 10](#_Toc435301753)

[7.4 Network Configuration 11](#_Toc435301754)

[7.5 System 12](#_Toc435301755)

[7.6 User Handling 13](#_Toc435301756)

[7.7 Event handling 14](#_Toc435301757)

[7.8 Video Streaming 16](#_Toc435301758)

[7.9 Video Streaming – MJPEG 17](#_Toc435301759)

[7.10 Video Encoder Configuration 18](#_Toc435301760)

[7.11 Media Profile Configuration 19](#_Toc435301761)

[7.12 Video Source Configuration 20](#_Toc435301762)

[7.13 Metadata Configuration 21](#_Toc435301763)

[8 Profile Conditional Features (normative) 22](#_Toc435301764)

[8.1 Video Streaming – MPEG4 (if supported) 22](#_Toc435301765)

[8.2 Video Streaming – H264 (if supported) 23](#_Toc435301766)

[8.3 PTZ (if supported) 24](#_Toc435301767)

[8.4 PTZ – Absolute Positioning (if supported) 26](#_Toc435301768)

[8.5 PTZ – Relative Positioning (if supported) 27](#_Toc435301769)

[8.6 PTZ – Presets (if supported) 28](#_Toc435301770)

[8.7 PTZ – Home Position (if supported) 29](#_Toc435301771)

[8.8 PTZ – Auxiliary Command (if supported) 30](#_Toc435301772)

[8.9 Audio Streaming (if supported) 31](#_Toc435301773)

[8.10 Audio Streaming – G726 (if supported) 32](#_Toc435301774)

[8.11 Audio Streaming – AAC (if supported) 33](#_Toc435301775)

[8.12 Multicast Streaming (if supported) 34](#_Toc435301776)

[8.13 Relay Outputs (if supported) 35](#_Toc435301777)

[8.14 NTP (if supported) 36](#_Toc435301778)

[8.15 Dynamic DNS (if supported) 37](#_Toc435301779)

[8.16 Zero Configuration (if supported) 38](#_Toc435301780)

[8.17 IP Address Filtering (if supported) 39](#_Toc435301781)

[9 Device Discovery 40](#_Toc435301782)

[9.1 Types 40](#_Toc435301783)

# Scope

This document defines the mandatory and conditional features required by an ONVIF Device and ONVIF Client that support the Profile S.

# Normative references

This section defines the normative references applicable to this specification.

## Normative References

* ONVIF Profile Policy

< <http://www.onvif.org/imwp/download.asp?ContentID=20983> >

* ONVIF Network Interface Specification Set

< <http://www.onvif.org/Documents/Specifications.aspx> >

# Terms and Definitions

This section provides common terms and definitions used in this specification.

## Definitions

|  |  |
| --- | --- |
| **Profile** | See [ONVIF Profile Policy]. |
| **ONVIF Device** | Networked hardware appliance or software program that exposes one or multiple ONVIF Web Services |
| **ONVIF Client** | Networked hardware appliance or software program that uses ONVIF Web Services. |

# Technical Specification Version Requirement

Implementation of ONVIF Network Interface Specification Set, version 1.02 or later is required for conformance to Profile S.

# Requirement Levels

Each feature in this document has a requirement level for Device and Client that claim conformance to Profile S and contains a Function List that states the functions requirement level for Device and Client that implement that feature.

The requirement levels for features are:

* Mandatory = Feature that shall be implemented by an ONVIF device or ONVIF client.
* Conditional = Feature that shall be implemented by an ONVIF device or ONVIF client if it supports that functionality in any way, including any proprietary way. Features that are conditional are marked with “if supported” in a profile specification.

The requirement levels for functions are:

* Mandatory = Function that shall be implemented by an ONVIF device or ONVIF client.
* Conditional = Function that shall be implemented by an ONVIF device or ONVIF client if it supports that functionality.
* Optional = Function that may be implemented by an ONVIF device or ONVIF client.

Function Lists use the following abbreviations:

* M = Mandatory
* C = Conditional
* O = Optional

All functions shall be implemented as described in the corresponding [ONVIF Network Interface Specification Set].

# Overview

An ONVIF device compliant to the Profile S is an ONVIF device that sends video data over an IP network to a client. The Profile S also includes support for PTZ, audio and metadata streaming, and relay outputs if those features are present on the device. For example, a device compliant to the Profile S may be an IP network camera or an encoder device.

An ONVIF client compliant to the Profile S is an ONVIF client that can configure, request, and control streaming of video data over an IP network from an ONVIF device compliant to the Profile S. The Profile S also includes support for control of PTZ, receiving audio and metadata stream, and relay outputs if those features are supported by the client.

An ONVIF profile is described by a fixed set of functionalities through a number of services that are provided by the ONVIF standard. A number of services and functionalities are mandatory for each type of ONVIF profile. An ONVIF device and client may support any combination of profiles and other optional services and functionalities.

# Profile Mandatory Features (normative)

Devices and Clients conformant to Profile S shall support the following features.

## User Authentication

* WS-Usernametoken using timestamps and nonce
* HTTP Digest

### Device requirements

* Device shall support WS-Usernametoken according to WS-Security as covered by the Core Specification.

### Client requirements

* Client shall implement WS-Usernametoken according to WS-security as covered by the core specification.
* Client shall implement HTTP Digest as covered by the core specification.

### User authentication Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **User Authentication** | | **Device MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| WS-Usernametoken Authentication | Core | M |
| HTTP Digest | Core | O |

### User authentication Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **User Authentication** | | **Client MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| WS-Usernametoken Authentication | Core | M |
| HTTP Digest | Core | M |

## 

## Capabilities

* Querying device for capabilities.

### Device requirements

* Capabilities and WSDL URL operations as detailed in the Core Specification.

### Client requirements

* Client shall be able to get Capabilities of a device using GetCapabilities.

### Capabilities Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Capabilities** | | **Device MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| GetCapabilities | Device | M |
| GetWsdlUrl | Device | M |

### Capabilities Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Capabilities** | | **Client MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| GetCapabilities | Device | M |
| GetWsdlUrl | Device | O |

## Discovery

* Discovery of a device on the network.
* Setting of discovery mode.
* Listing, adding, modifying and removing of discovery scopes.

### Device requirements

* WS-Discovery as covered by the core specification.
* Discovery configuration and scope operations as covered by the device service.

### Client requirements (if supported)

* Client shall be able to discover a device using WS-Discovery as specified in the core specification.

### Discovery Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Discovery** | | **Device MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| WS-Discovery | Core | M |
| GetDiscoveryMode | Device | M |
| SetDiscoveryMode | Device | M |
| GetScopes | Device | M |
| SetScopes | Device | M |
| AddScopes | Device | M |
| RemoveScopes | Device | M |

### Discovery Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Discovery** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| WS-Discovery | Core | M |
| GetDiscoveryMode | Device | O |
| SetDiscoveryMode | Device | O |
| GetScopes | Device | O |
| SetScopes | Device | O |
| AddScopes | Device | O |
| RemoveScopes | Device | O |

## Network Configuration

* Configuration of network settings on the device.

### Device requirements

* Device shall support Hostname, DNS, network interface, network protocol and network default gateway operations as covered by the device service.

### Client requirements (if supported)

* If configuring a device’s network configuration is supported in any way by the client, the client shall be able to list and configure the device network interface using the GetNetworkInterfaces and SetNetworkInterfaces operations.
* If configuring a device’s network configuration is supported in any way by the client, the client shall be able to list and set the default gateway of the device using the GetNetworkDefaultGateway and SetNetworkDefaultGateway operations.

### Network Configuration Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Network Configuration** | | **Device MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| GetHostname | Device | M |
| SetHostname | Device | M |
| GetDNS | Device | M |
| SetDNS | Device | M |
| GetNetworkInterfaces | Device | M |
| SetNetworkInterfaces | Device | M |
| GetNetworkProtocols | Device | M |
| SetNetworkProtocols | Device | M |
| GetNetworkDefaultGateway | Device | M |
| SetNetworkDefaultGateway | Device | M |

### Network Configuration Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Network Configuration** | | **Client CONDITIONAL** | |
|  | **Function** | **Device** | **Requirement** |
| GetHostname | Device | O |
| SetHostname | Device | O |
| GetDNS | Device | O |
| SetDNS | Device | O |
| GetNetworkInterfaces | Device | M |
| SetNetworkInterfaces | Device | M |
| GetNetworkProtocols | Device | O |
| SetNetworkProtocols | Device | O |
| GetNetworkDefaultGateway | Device | M |
| SetNetworkDefaultGateway | Device | M |

## System

* Configuration of system settings.
* Device information.

### Device requirements

* Device shall support get information, date and time, factory defaults and reboot operations as covered by the device service.

### Client requirements (if supported)

* Client shall be able to get device information such as manufacturer, model and firmware version using the GetDeviceInformation operation.

### System Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **System** | | **Device MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| GetDeviceInformation | Device | M |
| GetSystemDateAndTime | Device | M |
| SetSystemDateAndTime | Device | M |
| SetSystemFactoryDefault | Device | M |
| Reboot | Device | M |

### System Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **System** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetDeviceInformation | Device | M |
| GetSystemDateAndTime | Device | O |
| SetSystemDateAndTime | Device | O |
| SetSystemFactoryDefault | Device | O |
| Reboot | Device | O |

## User Handling

* Manage users on the device.

### Device requirements

* Device shall support user handling operations as covered by the device service.

### Client requirements (if supported)

* Client shall be able to create, list, modify and delete users from the device using the CreateUsers, GetUsers, SetUser and DeleteUsers operations.

### User Handling Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **User Handling** | | **Device MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| GetUsers | Device | M |
| CreateUsers | Device | M |
| DeleteUsers | Device | M |
| SetUser | Device | M |

### User Handling Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **User Handling** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetUsers | Device | M |
| CreateUsers | Device | M |
| DeleteUsers | Device | M |
| SetUser | Device | M |

## Event handling

* Retrieving and filtering of events from a device

### Device Requirements

* WS-BaseNotification as covered by the event service.
* Event and pull point operations as covered by the event service.

### Client Requirements (if supported)

* Client shall be able to use at least one way to retrieve events out of the following:
  + “Pull” using the CreatePullPointSubscription and PullMessage operations.
  + “Push” using Notify, Subscribe and Renew operations from WS-BaseNotification.

### Event Handling Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Event Handling** | | **Device MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| Notify | Event | M |
| Subscribe | Event | M |
| Renew | Event | M |
| Unsubscribe | Event | M |
| SetSynchronizationPoint | Event | M |
| CreatePullPointSubscription | Event | M |
| PullMessages | Event | M |
| GetEventProperties | Event | M |
| TopicFilter | Event | M |
| MessageContentFilter | Event | M |

### Event Handling Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Event Handling** | | **Client Conditional** | |
|  | **Function** | **Service** | **Requirement** |
| Notify | Event | M\* |
| Subscribe | Event |
| Renew | Event |
| Unsubscribe | Event | O |
| SetSynchronizationPoint | Event | O |
| CreatePullPointSubscription | Event | M\* |
| PullMessages | Event |
| GetEventProperties | Event | O |
| TopicFilter | Event | O |
| MessageContentFilter | Event | O |

\*Client shall implement one or both from PullPoint and Base-Notification to support Event Handling.

## Video Streaming

* Listing of media profiles
* Streaming of video using RTSP

### Device Requirements

* At least one ready-to-use Media Profile for Video Streaming
* Stream URI and profile operations as covered by the media service.
* Media streaming over RTSP as covered by the streaming specification.

### Client Requirements

* Client shall be able to list media profiles from the device using the GetProfiles operation.
* Client shall be able to get the stream URI for the selected profile using the GetStreamURI operation.
* Client shall be able to stream video on RTP/UDP or RTP/RTSP/HTTP/TCP using the selected profile over RTSP.

### Video Streaming Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Video Streaming** | | **Device MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| GetProfiles | Media | M |
| GetStreamUri | Media | M |
| Media Streaming using RTSP | Streaming | M |

### Video Streaming Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Video Streaming** | | **Client MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| GetProfiles | Media | M |
| GetStreamUri | Media | M |
| Media Streaming using RTSP | Streaming | M |

## 

## Video Streaming – MJPEG

* Streaming of MJPEG video using RTSP.
* Sub-feature of 7.1 Video Streaming.

### Device requirements

* Device shall declare MJPEG Option in VideoEncoderConfigurationOptions.
* Device shall be able to stream MJPEG according to the Streaming Specification.

### Client requirements

* Client shall be able to receive a stream and decode MJPEG video using the selected profile over RTSP.
* Client shall be able to understand RTSP – JPEG RTP header extension.

### Video Streaming – MJPEG Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Video Streaming – MJPEG** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| Media Streaming using RTSP - JPEG RTP header extension | Streaming | C |

### Video Streaming – MJPEG Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Video Streaming – MJPEG** | | **Client MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| Media Streaming using RTSP - JPEG RTP header extension | Streaming | M |

## 

## Video Encoder Configuration

* Listing and modification of video encoder configurations on the device.

### Device requirements

* The device shall return its capabilities for the maximum number of concurrent streams in GetGuaranteedNumberOfVideoEncoderInstances response.
* Video encoder configuration operations as covered by the media service.

### Client requirements

* Client shall be able to modify video encoder configurations using the GetVideoEncoderConfigurationOptions and SetVideoEncoderConfiguration operations.

### Video Encoder Configuration Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Video Encoder Configuration** | | **Device MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| GetVideoEncoderConfiguration | Media | M |
| GetVideoEncoderConfigurations | Media | M |
| AddVideoEncoderConfiguration | Media | M |
| RemoveVideoEncoderConfiguration | Media | M |
| SetVideoEncoderConfiguration | Media | M |
| GetCompatibleVideoEncoderConfigurations | Media | M |
| GetVideoEncoderConfigurationOptions | Media | M |
| GetGuaranteedNumberOfVideoEncoderInstances | Media | M |

### Video Encoder Configuration Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Video Encoder Configuration** | | **Client MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| GetVideoEncoderConfiguration | Media | O |
| GetVideoEncoderConfigurations | Media | O |
| AddVideoEncoderConfiguration | Media | O |
| RemoveVideoEncoderConfiguration | Media | O |
| SetVideoEncoderConfiguration | Media | M |
| GetCompatibleVideoEncoderConfigurations | Media | O |
| GetVideoEncoderConfigurationOptions | Media | M |
| GetGuaranteedNumberOfVideoEncoderInstances | Media | O |

## Media Profile Configuration

* Creation, retrieval and deletion of media profiles

### Device requirements

* Media profile operations as covered by the media service

### Client requirements (if supported)

* Client shall be able to list available profiles using the GetProfiles operation.
* Client shall be able to create a media profile using the CreateProfile operation.

### Media Profile Configuration Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Media Profile Configuration** | | **Device MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| GetProfiles | Media | M |
| GetProfile | Media | M |
| CreateProfile | Media | M |
| DeleteProfile | Media | M |

### Media Profile Configuration Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Media Profile Configuration** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetProfiles | Media | M |
| GetProfile | Media | O |
| CreateProfile | Media | M |
| DeleteProfile | Media | O |

## Video Source Configuration

* Listing and modification of video source configurations on the device.

### Device requirements

* Video source and video source configuration operations as covered by the media service.

### Client requirements (if supported)

* Client shall be able to modify and add video source configurations using the GetCompatibleVideoSourceConfigurations, GetVideoSourceConfigurationOptions, SetVideoSourceConfiguration and AddVideoSourceConfiguration operations.

### Video Source Configuration Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Video Source Configuration** | | **Device MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| GetVideoSources | Media | M |
| GetVideoSourceConfiguration | Media | M |
| GetVideoSourceConfigurations | Media | M |
| AddVideoSourceConfiguration | Media | M |
| RemoveVideoSourceConfiguration | Media | M |
| SetVideoSourceConfiguration | Media | M |
| GetCompatibleVideoSourceConfigurations | Media | M |
| GetVideoSourceConfigurationOptions | Media | M |

### Video Source Configuration Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Video Source Configuration** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetVideoSources | Media | O |
| GetVideoSourceConfiguration | Media | O |
| GetVideoSourceConfigurations | Media | O |
| AddVideoSourceConfiguration | Media | M |
| RemoveVideoSourceConfiguration | Media | O |
| SetVideoSourceConfiguration | Media | M |
| GetCompatibleVideoSourceConfigurations | Media | M |
| GetVideoSourceConfigurationOptions | Media | M |

## Metadata Configuration

* Listing and modification of metadata configuration on the device.

### Device requirements

* Metadata configuration operations as covered by the media service.

### Client requirements (if supported)

* Client shall be able to modify metadata configurations using the, GetMetaDataConfigurationOptions and SetMetaDataConfiguration operations.

### Metadata Configuration Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Metadata Configuration** | | **Device MANDATORY** | |
|  | **Function** | **Service** | **Requirement** |
| GetMetadataConfiguration | Media | M |
| GetMetadataConfigurations | Media | M |
| AddMetadataConfiguration | Media | M |
| RemoveMetadataConfiguration | Media | M |
| SetMetadataConfiguration | Media | M |
| GetCompatibleMetadataConfigurations | Media | M |
| GetMetadataConfigurationOptions | Media | M |

### Metadata Configuration Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Metadata Configuration** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetMetadataConfiguration | Media | O |
| GetMetadataConfigurations | Media | O |
| AddMetadataConfiguration | Media | O |
| RemoveMetadataConfiguration | Media | O |
| SetMetadataConfiguration | Media | M |
| GetCompatibleMetadataConfigurations | Media | O |
| GetMetadataConfigurationOptions | Media | M |

# Profile Conditional Features (normative)

The Profile Conditional Features section list the features that shall be implemented if the device or client supports the feature. For instance a device implementing Firmware Update in the native API shall also implement the ONVIF Firmware Update interface as specified in the [ONVIF Network Interface Specification Set]. The requirements represent the minimum functionality that must be implemented for conformance.

## Video Streaming – MPEG4 (if supported)

* Streaming of MPEG4 video using RTSP.
* Sub-feature of Video Streaming.

### Device requirements (if supported)

* Device shall declare MPEG4 option in VideoEncoderConfigurationOptions.
* Device shall be able to stream MPEG4 according to the Streaming Specification.
* Device shall send a key frame on-demand upon reception of SetSynchronizationPoint request when streaming MPEG4.

### Client requirements (if supported)

* Client shall be able to receive a stream and decode MPEG4 video using the selected profile over RTSP.

### Video Streaming – MPEG4 Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Video Streaming – MPEG4** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| SetSynchronizationPoint | Media | M |

### Video Streaming – MPEG4 Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Video Streaming – MPEG4** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| SetSynchronizationPoint | Media | O |

## Video Streaming – H264 (if supported)

* Streaming of H264 video using RTSP
* Sub-feature of Video Streaming

### Device requirements (if supported)

* Device shall declare H264 option in VideoEncoderConfigurationOptions.
* Device shall be able to stream H264 according to the Streaming Specification.
* Device shall send a key frame on-demand upon reception of SetSynchronizationPoint request when streaming H264.

### Client requirements (if supported)

* Client shall be able to receive a stream and decode H264 video using the selected profile over RTSP.

### Video Streaming – H264 Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Video Streaming – H264** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| SetSynchronizationPoint | Media | M |

### Video Streaming – H264 Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Video Streaming – H264** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| SetSynchronizationPoint | Media | O |

## 

## PTZ (if supported)

* Moving and stopping a PTZ device using continuous move.

### Device requirements (if supported)

* Device shall return PTZ capabilities in GetCapabilities response.
* Device shall return its PTZ status in GetStatus response.
* Continuous Move and Stop operations, and Continuous Velocity Spaces as covered by the PTZ service.
* Device shall expose all its PTZ Nodes via the GetNodes and GetNode operation.
* PTZ configuration operations as covered by the media service and the PTZ service.

### Client requirements (if supported)

* Client shall be able to read PTZ capabilities from a PTZ node using GetNodes or GetNode operations.
* Client shall be able to add a PTZ configuration to a profile using GetConfigurations and AddPTZConfiguration.
* Client shall be able to move a PTZ device using the ContinuousMove operation.
* Client shall be able to stop a PTZ device using the Stop operation.

### PTZ Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **PTZ** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| AddPTZConfiguration | Media | M |
| RemovePTZConfiguration | Media | M |
| GetNodes | PTZ | M |
| GetNode | PTZ | M |
| GetConfigurations | PTZ | M |
| GetConfiguration | PTZ | M |
| GetConfigurationOptions | PTZ | M |
| SetConfiguration | PTZ | M |
| ContinuousMove | PTZ | M |
| Stop | PTZ | M |
| GetStatus | PTZ | M |

### PTZ Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **PTZ** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| AddPTZConfiguration | Media | M |
| RemovePTZConfiguration | Media | O |
| GetNodes | PTZ | M |
| GetNode | PTZ | M |
| GetConfigurations | PTZ | M |
| GetConfiguration | PTZ | O |
| GetConfigurationOptions | PTZ | O |
| SetConfiguration | PTZ | O |
| ContinuousMove | PTZ | M |
| Stop | PTZ | M |
| GetStatus | PTZ | O |

## 

## PTZ – Absolute Positioning (if supported)

* Moving a PTZ device to an absolute position.
* Sub-feature of PTZ.

### Device requirements (if supported)

* AbsoluteMove operation, Absolute Position and Generic Speed Spaces as covered by the PTZ service.

### Client requirements (if supported)

* Client shall be able to move a PTZ device using the AbsoluteMove operation.

### PTZ – Absolute Positioning Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **PTZ – Absolute Positioning** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| AbsoluteMove | PTZ | M |

### PTZ – Absolute Positioning Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **PTZ – Absolute Positioning** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| AbsoluteMove | PTZ | M |

## 

## PTZ – Relative Positioning (if supported)

* Moving a PTZ device to a relative position.
* Sub-feature of PTZ.

### Device requirements (if supported)

* RelativeMove operation, Relative Translation and Generic Speed Spaces as covered by the PTZ service.

### Client requirements (if supported)

* Client shall be able to move a PTZ device using the RelativeMove operation.

### PTZ – Relative Positioning Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **PTZ – Relative Positioning** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| RelativeMove | PTZ | M |

### PTZ – Relative Positioning Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **PTZ – Relative Positioning** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| RelativeMove | PTZ | M |

## 

## PTZ – Presets (if supported)

* Listing of presets.
* Moving a PTZ device to a preset.
* Sub-feature of PTZ.

### Device requirements (if supported)

* A PTZ node with the MaximumNumberOfPresets capability set to at least 1.
* Preset operations as covered by the PTZ service.

### Client requirements (if supported)

* Client shall be able to list the presets using the GetPresets operation.
* Client shall be able to move a PTZ device to a specific preset using the GotoPreset operation.

### PTZ – Presets Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **PTZ – Presets** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| SetPreset | PTZ | M |
| GetPresets | PTZ | M |
| GotoPreset | PTZ | M |
| RemovePreset | PTZ | M |

### PTZ – Presets Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **PTZ – Presets** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| SetPreset | PTZ | O |
| GetPresets | PTZ | M |
| GotoPreset | PTZ | M |
| RemovePreset | PTZ | O |

## 

## PTZ – Home Position (if supported)

* Moving a PTZ device to its home position.
* Sub-feature of PTZ.

### Device requirements (if supported)

* A PTZ node with the HomeSupported capability set to “true”.
* Home position operations as covered by the PTZ service.

### Client requirements (if supported)

* Client shall be able to move a PTZ device to its home position using the GotoHomePosition operation.

### PTZ – Home Position Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **PTZ – Home Position** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GotoHomePosition | PTZ | M |
| SetHomePosition | PTZ | C |

### PTZ – Home Position Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **PTZ – Home Position** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GotoHomePosition | PTZ | M |
| SetHomePosition | PTZ | O |

## 

## PTZ – Auxiliary Command (if supported)

* Support for PTZ specific auxiliary commands.
* Sub-feature of PTZ.

### Device requirements (if supported)

* A PTZ node containing a non-empty list of auxiliary commands in the AuxiliaryCommands capability.
* Auxiliary command operation as covered by the PTZ service.

### Client requirements (if supported)

* Client shall be able to send auxiliary command to a PTZ device using the SetAuxiliaryCommand operation.

### PTZ – Auxiliary Command Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **PTZ – Auxiliary Command** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| SendAuxiliaryCommand | PTZ | M |

### PTZ – Auxiliary Command Position Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **PTZ – Auxiliary Command** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| SendAuxiliaryCommand | PTZ | M |

## 

## Audio Streaming (if supported)

* Streaming of Audio.

### Device requirements (if supported)

* Device shall declare G711 option in AudioEncoderConfigurationOptions.
* Device shall be able to stream G711 according to the Streaming Specification.
* Audio source, audio source configuration and audio encoder configuration operations as covered by the media service.

### Client requirements (if supported)

* Client shall be able to receive a stream and playback audio in G.711μ Law (Simplex-Camera Microphone Only, 1ch) codec.
* Client shall be able to configure a media profile for audio streaming using the GetCompatibleAudioSourceConfigurations, AddAudioSourceConfiguration, GetCompatibleAudioEncoderConfigurations, and AddAudioEncoderConfiguration operations.

### Audio Streaming Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Audio Streaming** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetAudioSources | Media | M |
| GetAudioSourceConfiguration | Media | M |
| GetAudioSourceConfigurations | Media | M |
| AddAudioSourceConfiguration | Media | M |
| RemoveAudioSourceConfiguration | Media | M |
| SetAudioSourceConfiguration | Media | M |
| GetCompatibleAudioSourceConfigurations | Media | M |
| GetAudioSourceConfigurationOptions | Media | M |
| GetAudioEncoderConfiguration | Media | M |
| GetAudioEncoderConfigurations | Media | M |
| AddAudioEncoderConfiguration | Media | M |
| RemoveAudioEncoderConfiguration | Media | M |
| SetAudioEncoderConfiguration | Media | M |
| GetCompatibleAudioEncoderConfigurations | Media | M |
| GetAudioEncoderConfigurationOptions | Media | M |

### Audio Streaming Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Audio Streaming** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetAudioSources | Media | O |
| GetAudioSourceConfiguration | Media | O |
| GetAudioSourceConfigurations | Media | O |
| AddAudioSourceConfiguration | Media | M |
| RemoveAudioSourceConfiguration | Media | O |
| SetAudioSourceConfiguration | Media | O |
| GetCompatibleAudioSourceConfigurations | Media | M |
| GetAudioSourceConfigurationOptions | Media | O |
| GetAudioEncoderConfiguration | Media | O |
| GetAudioEncoderConfigurations | Media | O |
| AddAudioEncoderConfiguration | Media | M |
| RemoveAudioEncoderConfiguration | Media | O |
| SetAudioEncoderConfiguration | Media | O |
| GetCompatibleAudioEncoderConfigurations | Media | M |
| GetAudioEncoderConfigurationOptions | Media | O |

## Audio Streaming – G726 (if supported)

* Streaming of G726 audio using RTSP
* Sub-feature of Audio Streaming

### Device requirements (if supported)

* Device shall declare G726 option in AudioEncoderConfigurationOptions.
* Device shall be able to stream G726 according to the Streaming Specification.

### Client requirements (if supported)

* Client shall be able to receive a stream and decode G726 audio using the selected profile over RTSP.

### Audio Streaming – G726 Function List for Devices

**No specific function requirement in addition to those listed in 8.9.3.**

### Audio Streaming – G726 Function List for Clients

**No specific function requirement in addition to those listed in 8.9.4.**

## Audio Streaming – AAC (if supported)

* Streaming of AAC audio using RTSP
* Sub-feature of Audio Streaming

### Device requirements (if supported)

* Device shall declare AAC option in AudioEncoderConfigurationOptions.
* Device shall be able to stream AAC according to the Streaming Specification.

### Client requirements (if supported)

* Client shall be able to receive a stream and decode AAC audio using the selected profile over RTSP.

### Audio Streaming – AAC Function List for Devices

**No specific function requirement in addition to those listed in 8.9.3.**

### Audio Streaming – AAC Function List for Clients

**No specific function requirement in addition to those listed in 8.9.4.**

## Multicast Streaming (if supported)

* Streaming video over multicast.
* Sub-feature of Video Streaming.

### Device requirements (if supported)

* Device shall return Media->Streaming->RTPMulticast capability set to “true” in GetCapabilities response.
* Multicast streaming operations as covered by the media service.

### Client requirements (if supported)

* Client shall be able to control multicast streaming using RTSP or the StartMultiCastStreaming and StopMultiCastStreaming operations.
* Client shall be able to receive a multicast stream sent by a device.

### Multicast Streaming Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Multicast Streaming** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| StartMulticastStreaming | Media | M |
| StopMulticastStreaming | Media | M |

### Multicast Streaming Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Multicast Streaming** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| StartMulticastStreaming | Media | C |
| StopMulticastStreaming | Media | C |

## 

## Relay Outputs (if supported)

* Listing, configuration and triggering of relay outputs

### Device requirements (if supported)

* Device shall return Device->IO->RelayOutputs capability set to at least 1 in GetCapabilities response.
* Relay output operations as covered by the device service.

### Client requirements (if supported)

* Client shall be able to list available relay outputs using the GetRelayOutputs operation.
* Client shall be able to set the settings of a relay output using the SetRelayOutputSettings operation.
* Client shall be able to trigger a relay output using the SetRelayOutputState operation.

### Relay Outputs Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Relay Outputs** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetRelayOutputs | Device | M |
| SetRelayOutputSettings | Device | M |
| SetRelayOutputState | Device | M |

### Relay Outputs Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Relay Outputs** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetRelayOutputs | Device | M |
| SetRelayOutputSettings | Device | M |
| SetRelayOutputState | Device | M |

## 

## NTP (if supported)

* Synchronization of time using NTP servers.

### Device requirements (if supported)

* NTP operations as covered by the device service.

### Client requirements (if supported)

* Client shall be able to configure NTP servers on a device using GetNTP and SetNTP operations.

### NTP Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **NTP** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetNTP | Device | M |
| SetNTP | Device | M |

### NTP Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **NTP** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetNTP | Device | M |
| SetNTP | Device | M |

## 

## Dynamic DNS (if supported)

* Configuration of Dynamic DNS.

### Device requirements (if supported)

* Device shall return Device->Network->DynDNS capability set to “true” in GetCapabilities response.
* Dynamic DNS operations as covered by the device service.

### Client requirements (if supported)

* Client shall be able to configure Dynamic DNS on device using GetDynamicDNS and SetDynamicDNS operations.

### Dynamic DNS Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Dynamic DNS** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetDynamicDNS | Device | M |
| SetDynamicDNS | Device | M |

### Dynamic DNS Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Dynamic DNS** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetDynamicDNS | Device | M |
| SetDynamicDNS | Device | M |

## 

## Zero Configuration (if supported)

* Configuration of Zero Configuration.

### Device requirements (if supported)

* Device shall return Device->Network->ZeroConfiguration capability set to “true” in GetCapabilities response.
* Zero Configuration operations as covered by the device service.

### Client requirements (if supported)

* Client shall be able to configure Zero Configuration on device using GetZeroConfiguration and SetZeroConfiguration operations.

### Zero Configuration Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Zero Configuration** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetZeroConfiguration | Device | M |
| SetZeroConfiguration | Device | M |

### Zero Configuration Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Zero Configuration** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetZeroConfiguration | Device | M |
| SetZeroConfiguration | Device | M |

## 

## IP Address Filtering (if supported)

* Configuration of IP Address Filters.

### Device requirements (if supported)

* Device shall return Device->Network->IPFilter capability set to “true” in GetCapabilities response.
* IP Address Filter operations as covered by the device service.

### Client requirements (if supported)

* Client shall be able to configure, add and remove IP Address Filters on device using GetIPAddressFilter, SetIPAddressFilter, AddIPAddressFilter and RemoveIPAddressFilter operations.

### Relay Outputs Function List for Devices

|  |  |  |  |
| --- | --- | --- | --- |
| **Relay Outputs** | | **Device CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetIPAddressFilter | Device | M |
| SetIPAddressFilter | Device | M |
| AddIPAddressFilter | Device | M |
| RemoveIPAddressFilter | Device | M |

### Relay Outputs Function List for Clients

|  |  |  |  |
| --- | --- | --- | --- |
| **Relay Outputs** | | **Client CONDITIONAL** | |
|  | **Function** | **Service** | **Requirement** |
| GetIPAddressFilter | Device | M |
| SetIPAddressFilter | Device | M |
| AddIPAddressFilter | Device | M |
| RemoveIPAddressFilter | Device | M |

# Device Discovery

An ONVIF device shall implement device discovery as specified in the ONVIF Core Specification.

A device compliant to this specification shall additionally include the specific scope parameter as presented in Table 1: Scope parameters. Apart from this pre-defined parameter, it shall be possible to set any scope parameter as defined by the device owner. Scope parameters can be listed and set through the commands provided by the Device service, defined in the ONVIF Core Specification.

Table 1: Scope parameters

|  |  |  |
| --- | --- | --- |
| **Category** | **Defined values** | **Description** |
| Profile | Streaming | The Streaming scope indicates if the device is compliant to the Profile S. A device compliant to the Profile S shall include a scope entry with this value in its scope list. |

## Types

Section "Discovery definitions" of the ONVIF Core Specification defines a generic tds:Device for the <d:Types> declaration.

For backward compatibility reason a device compliant to this specification shall also include dn:NetworkVideoTransmitter in the <d:Types> declaration and it may omit tds:Device.